Title: 
Your Guide To Plastic Molding

Word Count:
707

Summary:
Plastics are synthetically produced non-metallic compounds. It can be molded into various forms and hardened for commercial use. Plastic molding products can be seen everywhere. Examples are jars, protective caps, plastic tubes, grips, toys, bottles, cases, accessories, kitchen utensils and a lot more. 

Even the keyboard and the mouse that you use are made through plastic molding. Even the plastic parts of the chair that you are sitting on are created this way. 

The bas...


Keywords:
plastic molding,injection molding


Article Body:
Plastics are synthetically produced non-metallic compounds. It can be molded into various forms and hardened for commercial use. Plastic molding products can be seen everywhere. Examples are jars, protective caps, plastic tubes, grips, toys, bottles, cases, accessories, kitchen utensils and a lot more. 

Even the keyboard and the mouse that you use are made through plastic molding. Even the plastic parts of the chair that you are sitting on are created this way. 

The basic idea in plastic molding is inserting molten liquid plastic into a ready shaped mold, for example the mold of a bottle. It will then be allowed to cool, then the mold will be removed to reveal the plastic bottle. 

Plastic molding can also custom-mold a wide variety of plastic products including: garden pots, cabinets, office trays and boxes, barriers, barricades and traffic signage and displays for product and marketing promotions. 

If you are planning to go into a plastic molding business, you should first know the different processes. Choose from a plastic molding process that fits your budget, your expertise, and your resources. Here are basic definitions of various methods of plastic molding. 

The Plastic Molding Processes: 

1. Injection Molding 

In Injection Molding, melted plastic is forced into a mold cavity. Once cooled, the mold can be removed. This plastic molding process is commonly used in mass-production or prototyping of a product. Injection molding machines were made in the 1930’s. This can be used to mass produce toys, kitchen utensils, bottle caps, and cell phone stands to name a few. 

2. Blow Molding 

Blow molding is like injection molding except that hot liquid plastic pours out of a barrel vertically in a molten tube. The mold closes on it and forces it outward to conform to the inside shape of the mold. When it is cooled, the hollow part is formed. Examples of blow molding products are bottles, tubes and containers. 

Equipments needed in setting-up a blow molding business are relatively higher than injection molding. 

3. Compression Molding 

In this type of plastic molding, a slug of hard plastic is pressed between two heated mold halves. Compression molding usually uses vertical presses instead of the horizontal presses used for injection and blow molding. The parts formed are then air-cooled. Prices of equipments used for compression molding are moderate. 

4. Film Insert Molding 

This plastic molding technique imbeds an image beneath the surface of a molded part. A material like film or fabric is inserted into a mold. Plastic is then injected. 

5. Gas Assist Molding 

Also called gas injection molding is used to create plastic parts with hollow interiors. Partial shot of plastic is then followed by high-pressure gas to fill the mold cavity with plastic. 

6. Rotational Molding 

Hollow molds packed with powdered plastic are secured to pipe-like spokes that extend from a central hub. The molds rotate on separate axes at once. The hub swings the whole mold to a closed furnace room causing the powder to melt and stick to the insides of the tools. As the molds turn slowly, the tools move into a cooling room. Here, sprayed water causes the plastic to harden into a hollow part. In this type of plastic molding, tooling costs are low and piece prices are high. Cycle time takes about 40-45 minutes. 

7. Structural Foam Molding 

Structural foam molding is a process of plastic molding usually used for parts that require thicker walls than standard injection molding. Inserting a small amount of nitrogen or chemical blow agent into the plastic material makes the walls thicker. Foaming happens as the melted plastic material enters the mold cavity. A thin plastic skin forms and solidifies in the mold wall. This type of plastic molding can be used with any thermoplastic that can be injection molded. 

8. Thermoforming 

In this plastic molding process, sheets of pre-extruded rigid plastics are horizontally heated and sucked down into hollow one-piece tools. When the hot plastic solidifies, its shape conforms to that of the mold. 

Tooling costs are usually low and piece prices vary on the machinery. 

Plastic molding is a very technical process. It needs experts in this type of manufacturing business for it to be competitive in the market. Therefore, a very scientific and systematic study should be first made before going into this endeavor.


