Auto Detailing And Car Paint Imperfections Removal

Since your car paint is the initial most evident feature of your car, then you need to invest enough time caring and maintaining for it to keep it looking as if it is brand new. Sadly though, a lot of car owners have fell victim to faulty paint jobs that make your car end up looking cheap and wasted. To remedy that, there are auto detailing services that specialize on removing and correcting imperfections in your car paint. 

Whether you are hiring a professional service for it or doing the fix yourself, below are some key information you need to know. 

Use of Fine Compound

The use of fine compound is often the default remedy for poor paint jobs. But before you proceed further, there are some scenarios wherein it is not allowed unless absolutely necessary. These include the following:

• wet spots and swirl marks
• micro marring
• paint repair blending 
• excessive sun exposure
• pitting from hard stones and sand 
• poor paint surface finish

Careful Detailing for Car Paint 

When detailing your car, the use of the right tools and products make a huge difference with the quality of results. But aside from the basic detailing materials, your hand is one of your best tools. Some automated detailing jobs can be too harsh as to cause damage on your car, more than you initially came in with. 

Make sure you take proper notes when preparing your compound. This is especially useful in removing scratches and faulty paint jobs. Avoid masking off the trim for it will only increase your job significantly. Make sure to use compounds in the same way as you would a sandpaper and avoid applying more than 2' by 2' in a given area. But if you would like to stick with spot treatment for scratches or uneven paint, then try to focus application of compound within that given area. 

Tips for Improved Compounding Results 

If you want to enhance the overall quality of your car paint, you need to consider applying the following tips for better compounding results:

• Apply a slight brush of detailing spray onto the polishing pad since it will make applying the compound a lot easier and more precise. Just keep it damp (not wet) using one quick shot.

• When applying paint on sharp edges of your car, make sure to apply it thinly. Avoid using compound on these areas.

• Use a dense foam applicator for the compound since it is much safer and easier to handle with better results.

• Avoid trying to lessen the appearance of any imperfection on the paint job, say a scratch. If it is not that noticeable, it would be better to leave it alone instead of ruining the entire paint job.

Fine Polish and Finish 

To completely eliminate any imperfections and give your car a new shine on its paint for a brand-new look, then you can add polish as the finishing touch. You need to understand though that this is done only for enhancement purposes, but will not fix any imperfections on your car paint. 

There are some basic hand car polishing techniques you need to learn to effectively perform this job. The main point behind car polishing is to create a finer texture on the paint surface prior to glazing. You won't need a sealant or wax to reveal the natural gloss of the paint. The secret tool here is a high quality foam applicator, which is very effective in buffing polish residue for a nearly perfect look. You will soon find out that it delivers a far more superior auto detailing result in the end. 
